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876 Eechomagnetic counter

50r 6-digit display, HXW 4mmx 1
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Without reset mechanism
=220V,AC:24-240V
5V-220V,AC:24-240V
it sk & ACS108/4, DC<20%/4
Counting speed AC< 10tiems/sec, DC<20times/sec
5.7 @ R439mm x 27.5mm
Opening size(BxH)39mm % 27.5mm
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Customized designs available as per clients” requirements
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